2.08:
  NEW: New command: "Note On/Off" and "Note Trigger".
2.07:
  NEW: When writing a file to the MC-5jr, mode will be changed to "PROGAM-MODE".
  IMP: Changed version to Major.Minor instead of Major.Minor.Revision
2.6.0:
  NEW: Entering menu on hardware gives you 4 options: load EEPROM, load PRG settings,
       load Scenes settings, Calibrate Expression Pedal
  NEW: Calibrating will show the range using leds instead of LCD.
  IMP: Deleted command "Tuner" since it's useless without an LCD.
2.5.1:
  BUG: Using PC command wouldn't lit Led.
2.5.0:
  NEW: Press-Hold: Block Page. When using a page button, all buttons will switch 
       from Page 1 to Page2. Using Block Page will override this. Blocks with this 
       press-hold value will stay on Page 1.
  NEW: In Global tab, parameter "Bank select only on Midi Channel". 
       Commands Bank Up/Down/Select only affects the selected Midi Channel.
       If Midi Channel 0 is chosen, then Bank select will affect on every Midi Channel.
  NEW: Page button led shows active page (p1=blue/green p2=red)
  BUG: When Button is global. Global Button text is shown on Scene change. 
       Should be Scene text.
  BUG: Using more than one PC as command in a 'step-'button would not work when using
       global blocks.
  IMP: Adjusted form dimensions to fit on smaller screens.  
2.4.0:
  NEW: Global works now also on Scenes.
2.3.0:
  NEW: Expr 1 & 2 can now also be used as buttons using an external switch.
2.2.1:
  IMP: Minor improvements
2.2.0:
  NEW: Fractal Tuner now also available on page 2 or as press-and-hold
  IMP: Tuner button led will indicate if tuner is on/off
  IMP: When press-hold is set to "BLOCK", button will act faster (Midi messages send on 
       button engage instead of button release)
2.1.0:
  NEW: Fractal Tuner works now for Standard, Ultra, II, XL, XL+ and III
  MSC: When changing firmware, "Data needs to be updated!!" will be shown on reboot
       instead of "Caution! EEPROM Checksum Error" which was confusing
2.0.1: 
  BUG: Preset Down/Up Led stays on, should only blink
2.0.0:
  Initial firmware
