********************
*                  *
* firmware_MC-MIDI *
*                  *
********************
2.09:
  IMP: Interchanged tuner arrows >>> and <<<, which makes more sense.
2.08:
  NEW: Fractal Tuner works for Standard, Ultra, II, XL, XL+ and III.
2.07:
  NEW: New command: "Note On/Off" and "Note Trigger".
2.06:
  Editor: Removed MC-5jr. This product has his own firmware/editor.
  BUG: LCD displaying garbage.
  IMP: Changed version to Major.Minor instead of Major.Minor.Revision
2.5.1:
  BUG: Using PC command wouldn't lit Led.
2.5.0:
  NEW: Press-Hold: Block Page. When using a page button, all buttons will switch 
       from Page 1 to Page2. Using Block Page will override this. Blocks with this 
       press-hold value will stay on Page 1.
  NEW: In Global tab, parameter "Bank select only on Midi Channel". 
       Commands Bank Up/Down/Select only affects the selected Midi Channel.
       If Midi Channel 0 is chosen, then Bank select will affect on every Midi Channel.
  NEW: Page button led shows active page (p1=blue/green p2=red)
  BUG: When Button is global. Global Button text is shown on Scene change. 
       Should be Scene text.
  BUG: Using more than one PC as command in a 'step-'button would not work when using
       global blocks.
  IMP: Adjusted form dimensions to fit on smaller screens.  
2.4.0:
  NEW: Global works now also on Scenes.
2.3.0:
  NEW: Expr 1 & 2 can now also be used as buttons using an external switch.
2.2.1:
  IMP: Minor improvements
2.2.0:
  NEW: Fractal Tuner now also available on page 2 or as press-and-hold
  IMP: Tuner button led will indicate if tuner is on/off
  IMP: When press-hold is set to "BLOCK", button will act faster (Midi messages send on 
       button engage instead of button release)
2.1.0:
  NEW: Fractal Tuner works now for Standard, Ultra, II, XL, XL+ and III
  MSC: When changing firmware, "Data needs to be updated!!" will be shown on reboot
       instead of "Caution! EEPROM Checksum Error" which was confusing
2.0.1: 
  BUG: Preset Down/Up Led stays on, should only blink
2.0.0:
  Initial firmware

********************
*                  *
* firmware_MC-AFX2 *
*                  *
********************
1.03:
  NEW: Tempo light blinking.
  IMP: When MC Midi In is not connected to Axe-Fx II.
       Previously this would freeze the MC since it expects an answer from the Axe-Fx II.
       Now, the MC will still freeze, but the message "Time Out! Midi In Error" will be shown.
       Connect Midi In and reboot the MC.
  IMP: Interchanged tuner arrows >>> and <<<, which makes more sense.
1.02:
  Editor: Removed MC-5jr. This product has his own firmware/editor.
  IMP: Extend Preset range to 768.
  NEW: Show preset number.
  BUG: LCD displaying garbage.
  IMP: Changed version to Major.Minor instead of Major.Minor.Revision
1.1.1:
  IMP: Minor improvements
1.1.0:
  NEW: Fractal Tuner now also available on page 2 or as press-and-hold  
  IMP: Tuner button led will indicate if tuner is on/off
  IMP: When press-hold is set to "BLOCK", button will act faster (Midi messages send on 
       button engage instead of button release)
1.0.1:
  MSC: When changing firmware, "Data needs to be updated!!" will be shown on reboot
       instead of "Caution! EEPROM Checksum Error" which was confusing
1.0.0:
  Initial firmware  

************************
*                      *
* firmware_MC-AFX3_FM3 *
*                      *
************************
1.06:
  NEW: FM3 supported. 
  NEW: Tempo light blinking.
  IMP: When MC Midi In is not connected to III/FM3.
       Previously this would freeze the MC since it expects an answer from the III/FM3.
       Now, the MC will still freeze, but the message "Time Out! Midi In Error" will be shown.
       Connect Midi In and reboot the MC.
  IMP: Interchanged tuner arrows >>> and <<<, which makes more sense.
1.05:
  IMP: Rewrote Block syncing with Axe-Fx III.
1.04:
  Editor: Removed MC-5jr. This product has his own firmware/editor.
  BUG: LCD displaying garbage.
  IMP: Changed version to Major.Minor instead of Major.Minor.Revision
1.3.1:
  BUG: Scene led On when other page is selected.
1.3.0:
  NEW: Press-Hold: Block Page. When using a page button, all buttons will switch 
       from Page 1 to Page2. Using Block Page will override this. Blocks with this 
       press-hold value will stay on Page 1.
  NEW: Global - Show Preset # (Y/N).
  NEW: Page button led shows active page (p1=blue/green p2=red)
  BUG: Preset Up and Bank Up maximum was 382. Changed to 511.
  BUG: FX on page 2 (red) leds shown on page 1 on Scene or Preset change.
  BUG: When using Preset Select, selected button led is On.
1.2.0:
  IMP: Firmware adjusted to the New Fractal Midi Specs for reading Preset- and Scene-name.
       required: Axe-Fx III Firmware 1.15 Beta#2 or higher.
1.1.1:
  BUG: Preset Down/Up Led stayed on. Now led will blink briefly.
1.1.0:
  NEW: added block on/off. block-state will loaded on program or scene change
1.0.0:
  Initial firmware  

********************
*                  *
* firmware_MC-KMPR *
*                  *
********************
1.03:
  IMP: When MC Midi In is not connected to the Kemper.
       Previously this would freeze the MC since it expects an answer from the Kemper.
       Now, the MC will still freeze, but the message "Time Out! Midi In Error" will be shown.
       Connect Midi In and reboot the MC.
  IMP: Interchanged tuner arrows >>> and <<<, which makes more sense.
1.02:
  Editor: Removed MC-5jr. This product has his own firmware/editor.
  BUG: LCD displaying garbage.
  IMP: Changed version to Major.Minor instead of Major.Minor.Revision
1.1.0:
  Tuner info is shown on the LCD
1.0.0:
  Initial firmware  

